Rename the unforce_pulse4k.txt to force_pulse4k.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will then force the pulse4k-PurE2-7.4-20250828_mmc.zip into the linux1 slot
