Rename the unforce_hd61.txt to force_hd61.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will force to install the image ax61-PurE2-7.4-20250829_multi.zip in the linux1 selection
